Thu Apr 20, 2017 11:45:11: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:45:13: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:45:14: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:45:14: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:45:14: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:45:14: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:45:14: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:45:14: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:45:14: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:45:14: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:45:14: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:45:14: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:45:14: TPIU fitted.
Thu Apr 20, 2017 11:45:14: ETM fitted.
Thu Apr 20, 2017 11:45:14: ETB present.
Thu Apr 20, 2017 11:45:14: CSTF present.
Thu Apr 20, 2017 11:45:14: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:45:14: Initial reset was performed
Thu Apr 20, 2017 11:45:16: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 11:45:16: J-Link: Flash download: Total time needed: 0.387s (Prepare: 0.116s, Compare: 0.187s, Erase: 0.025s, Program: 0.050s, Verify: 0.000s, Restore: 0.007s)
Thu Apr 20, 2017 11:45:16: 93297 bytes downloaded (69.50 Kbytes/sec)
Thu Apr 20, 2017 11:45:16: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:45:16: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:45:16: Target reset
Thu Apr 20, 2017 11:47:27: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:47:45: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:47:46: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:47:46: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:47:46: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:47:46: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:47:46: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:47:46: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:47:46: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:47:46: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:47:46: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:47:46: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:47:46: TPIU fitted.
Thu Apr 20, 2017 11:47:46: ETM fitted.
Thu Apr 20, 2017 11:47:46: ETB present.
Thu Apr 20, 2017 11:47:46: CSTF present.
Thu Apr 20, 2017 11:47:47: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:47:47: Initial reset was performed
Thu Apr 20, 2017 11:47:48: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 11:47:48: J-Link: Flash download: Total time needed: 0.365s (Prepare: 0.095s, Compare: 0.185s, Erase: 0.025s, Program: 0.050s, Verify: 0.001s, Restore: 0.007s)
Thu Apr 20, 2017 11:47:48: 93297 bytes downloaded (71.24 Kbytes/sec)
Thu Apr 20, 2017 11:47:48: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:47:48: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:47:48: Target reset
Thu Apr 20, 2017 11:49:39: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)
Thu Apr 20, 2017 11:49:40: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:49:40: Target reset
Thu Apr 20, 2017 11:49:44: Breakpoint hit: Code @ app.c:226.6, type: default (auto) 
Thu Apr 20, 2017 11:49:44: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)
Thu Apr 20, 2017 11:49:54: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:50:32: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:50:33: Download complete.
Thu Apr 20, 2017 11:50:33: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:50:33: Target reset
Thu Apr 20, 2017 11:50:41: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:53:41: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:53:42: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:53:42: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:53:42: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:53:42: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:53:42: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:53:42: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:53:42: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:53:42: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:53:42: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:53:42: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:53:42: TPIU fitted.
Thu Apr 20, 2017 11:53:42: ETM fitted.
Thu Apr 20, 2017 11:53:42: ETB present.
Thu Apr 20, 2017 11:53:42: CSTF present.
Thu Apr 20, 2017 11:53:43: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:53:43: Initial reset was performed
Thu Apr 20, 2017 11:53:45: J-Link: Flash download: Flash programming performed for 2 ranges (4096 bytes)
Thu Apr 20, 2017 11:53:45: J-Link: Flash download: Total time needed: 0.460s (Prepare: 0.125s, Compare: 0.187s, Erase: 0.033s, Program: 0.102s, Verify: 0.002s, Restore: 0.008s)
Thu Apr 20, 2017 11:53:45: 93297 bytes downloaded (42.03 Kbytes/sec)
Thu Apr 20, 2017 11:53:45: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:53:45: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:53:45: Target reset
Thu Apr 20, 2017 11:53:52: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:55:10: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:55:10: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:55:10: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:55:10: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:55:10: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:55:10: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:55:10: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:55:10: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:55:10: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:55:10: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:55:10: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:55:10: TPIU fitted.
Thu Apr 20, 2017 11:55:10: ETM fitted.
Thu Apr 20, 2017 11:55:10: ETB present.
Thu Apr 20, 2017 11:55:10: CSTF present.
Thu Apr 20, 2017 11:55:11: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:55:11: Initial reset was performed
Thu Apr 20, 2017 11:55:13: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 11:55:13: J-Link: Flash download: Total time needed: 0.375s (Prepare: 0.107s, Compare: 0.183s, Erase: 0.025s, Program: 0.051s, Verify: 0.000s, Restore: 0.007s)
Thu Apr 20, 2017 11:55:13: 93297 bytes downloaded (61.48 Kbytes/sec)
Thu Apr 20, 2017 11:55:13: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:55:13: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:55:13: Target reset
Thu Apr 20, 2017 11:55:18: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:56:12: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:56:12: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:56:12: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:56:12: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:56:12: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:56:12: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:56:12: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:56:12: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:56:12: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:56:12: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:56:12: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:56:12: TPIU fitted.
Thu Apr 20, 2017 11:56:12: ETM fitted.
Thu Apr 20, 2017 11:56:12: ETB present.
Thu Apr 20, 2017 11:56:12: CSTF present.
Thu Apr 20, 2017 11:56:13: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:56:13: Initial reset was performed
Thu Apr 20, 2017 11:56:14: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 11:56:15: J-Link: Flash download: Total time needed: 0.370s (Prepare: 0.097s, Compare: 0.185s, Erase: 0.026s, Program: 0.050s, Verify: 0.000s, Restore: 0.009s)
Thu Apr 20, 2017 11:56:15: 93297 bytes downloaded (65.64 Kbytes/sec)
Thu Apr 20, 2017 11:56:15: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:56:15: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:56:15: Target reset
Thu Apr 20, 2017 11:57:08: The stack pointer for stack 'CSTACK' (currently 0x1FFFDCE0) is outside the stack range (0x1FFFF268 to 0x1FFFFA68)


 << Logging to file resumes >> 

Thu Apr 20, 2017 11:57:28: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 11:57:28: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 11:57:28: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 11:57:28: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 11:57:28: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 11:57:28: Selecting SWD as current target interface.

Thu Apr 20, 2017 11:57:28: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 11:57:28: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:57:28: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 11:57:28: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 11:57:28: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 11:57:28: TPIU fitted.
Thu Apr 20, 2017 11:57:28: ETM fitted.
Thu Apr 20, 2017 11:57:28: ETB present.
Thu Apr 20, 2017 11:57:28: CSTF present.
Thu Apr 20, 2017 11:57:29: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:57:29: Initial reset was performed
Thu Apr 20, 2017 11:57:30: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 11:57:30: J-Link: Flash download: Total time needed: 0.369s (Prepare: 0.097s, Compare: 0.187s, Erase: 0.025s, Program: 0.051s, Verify: 0.001s, Restore: 0.007s)
Thu Apr 20, 2017 11:57:30: 93297 bytes downloaded (68.71 Kbytes/sec)
Thu Apr 20, 2017 11:57:30: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 11:57:30: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 11:57:30: Target reset
Thu Apr 20, 2017 13:31:51: Failed to set breakpoint at 0x00011D96 (out of breakpoints?)
Thu Apr 20, 2017 13:31:52: Failed to set breakpoint at 0x00011D96 (out of breakpoints?)
Thu Apr 20, 2017 13:31:53: Failed to set breakpoint at 0x00011D96 (out of breakpoints?)
Thu Apr 20, 2017 13:31:53: Failed to set breakpoint at 0x00011D96 (out of breakpoints?)
Thu Apr 20, 2017 13:31:58: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:31:59: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:31:59: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:31:59: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:31:59: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:31:59: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:00: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:01: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:01: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:01: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:01: Failed to set breakpoint at 0x00011DF8 (out of breakpoints?)
Thu Apr 20, 2017 13:32:33: Fatal error:    Session aborted!


 << Logging to file resumes >> 

Thu Apr 20, 2017 13:32:39: Loaded macro file: D:\Program Files (x86)\IAR Systems\Embedded Workbench 7.0\arm\config\debugger\Freescale\Kxx.dmac
Thu Apr 20, 2017 13:32:39: JLINK command: ProjectFile = E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\settings\OS2_Debug.jlink, return = 0

Thu Apr 20, 2017 13:32:39: Device "MK60DN512XXX10" selected (512 KB flash, 128 KB RAM).
Thu Apr 20, 2017 13:32:39: DLL version: V4.86a, compiled Jun 11 2014 17:22:49

Thu Apr 20, 2017 13:32:39: Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52

Thu Apr 20, 2017 13:32:39: Selecting SWD as current target interface.

Thu Apr 20, 2017 13:32:39: JTAG speed is initially set to: 32 kHz
Thu Apr 20, 2017 13:32:39: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 13:32:39: Found SWD-DP with ID 0x2BA01477
Thu Apr 20, 2017 13:32:39: Found Cortex-M4 r0p0, Little endian.
Thu Apr 20, 2017 13:32:39: FPUnit: 6 code (BP) slots and 2 literal slots
Thu Apr 20, 2017 13:32:39: TPIU fitted.
Thu Apr 20, 2017 13:32:39: ETM fitted.
Thu Apr 20, 2017 13:32:39: ETB present.
Thu Apr 20, 2017 13:32:39: CSTF present.
Thu Apr 20, 2017 13:32:40: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 13:32:40: Initial reset was performed
Thu Apr 20, 2017 13:32:41: J-Link: Flash download: Flash programming performed for 1 range (2048 bytes)
Thu Apr 20, 2017 13:32:41: J-Link: Flash download: Total time needed: 0.368s (Prepare: 0.098s, Compare: 0.186s, Erase: 0.025s, Program: 0.050s, Verify: 0.000s, Restore: 0.007s)
Thu Apr 20, 2017 13:32:41: 93297 bytes downloaded (72.14 Kbytes/sec)
Thu Apr 20, 2017 13:32:41: Loaded debugee: E:\work\programm\Tunnel\trunk\mk60_ucos_lwip_01\PROJECT\Debug\Exe\OS2.out
Thu Apr 20, 2017 13:32:41: Hardware reset with strategy 0 was performed
Thu Apr 20, 2017 13:32:41: Target reset
